

**SURFACE MOUNTED PLEATED BLIND**

**ENQUIRY FORM**

**THIS ENQUIRY FOR IS FOR RECTANGLE OR SQUARE WINDOWS ONLY**

**THIS SYSTEM IS MANUALLY OPERATED AND NOT AVAILABLE AS A MOTORISED OPTION**

|  |  |
| --- | --- |
| Company Name |  |
| Contact Name |  |
| Telephone Number |  |
| Email Address |  |
| Vessel Name or Project Name |  |

Select the manual blind type (mark with a ‘x’) ‘SM’ refers to ‘Surface Mounted’

|  |  |
| --- | --- |
| SM Pleated Blind with SINGLE pleated material BLACKOUT SCREEN  A framed blind that has one single pleated blind that opens and closes |  |
| SM Pleated Blind with SINGLE pleated material DIMOUT SCREEN  A framed blind that has one single pleated blind that opens and closes |  |
| SM Pleated Blind with SINGLE pleated material INSECT SCREEN  A framed blind that has one single pleated blind that opens and closes |  |
| SM Pleated Blind with DOUBLE pleated material BLACKOUT SCREEN & DIMOUT SCREEN  A framed blind that has two pleated blinds that can be used separately or together |  |
| SM Pleated Blind with DOUBLE pleated material BLACKOUT SCREEN & INSECT SCREEN  A framed blind that has two pleated blinds that can be used separately or together |  |
| SM Pleated Blind with DOUBLE pleated material DIMOUT SCREEN & INSECT SCREEN  A framed blind that has two pleated blinds that can be used separately or together |  |

Select Colour of the profiles (mark with a ‘x’)

Only available as white

|  |  |
| --- | --- |
| White | **x** |

Select Colours (If a single screen tick one colour, if a double screen tick two colours)

|  |  |  |  |
| --- | --- | --- | --- |
| Atlanta FR Dimout WHITE |  | Atlanta FR Blackout SAND |  |
| Atlanta FR Dimout BEIGE |  | Atlanta FR Blackout WHITE |  |
| Atlanta FR Dimout FOSSIL |  | Atlanta FR Blackout BROWN |  |
| Atlanta FR Dimout DUST |  | Atlanta FR Blackout DUST |  |
| Atlanta FR Dimout SMOKE |  | Atlanta FR Blackout PEBBLE |  |
| Atlanta FR Dimout PEBBLE |  | Atlanta FR Blackout BLACK |  |
| Insect Screen BLACK |  |

**Collecting the Dimensions**

This blind is designed to fit over the top of a window that has no window box (recess) and that may have a frame that is slightly protruding. To ensure we get the size of the blind correct, simply provide us the size of the window glass + frame, we will then calculate the blind size from these dimensions. Bear in mind that the blind will be bigger than the dimensions provided, because its purpose is to cover the window with a snug fit. Note that this is only suitable for square or rectangular windows.

The unit is screwed directly into the surrounds, so no brackets are needed for this blind type

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Item | Qty | Window Ref | Width of window + frame | Height of Window glass + frame |
| 1 |  |  |  |  |
| 2 |  |  |  |  |
| 3 |  |  |  |  |
| 4 |  |  |  |  |
| 5 |  |  |  |  |
| 6 |  |  |  |  |
| 7 |  |  |  |  |
| 8 |  |  |  |  |
| 9 |  |  |  |  |
| 10 |  |  |  |  |

**Send to theteam@solarglide.com**